ND_RelParSet_K01 = {

Name = CR12MOV

PARAMETERS =
{
  Name = PTC_MATERIAL_DESCRIPTION
  Type = String
  Default = '冷冲模具钢，淬透性、淬火回火的硬度、耐磨性、强度均比Cr12高，
用于制造形状复杂、工作条件繁重下的冷冲模具和工具'
  Access = Full
},
{
  Name = TEMPERATURE
  Type = Real
  Default = 0.000000e+00 C
  Access = Full
},
{
  Name = PTC_INITIAL_BEND_Y_FACTOR
  Type = Real
  Default = 5.000000e-01
  Access = Full
},
{
  Name = PTC_BEND_TABLE
  Type = String
  Default = ''
  Access = Full
},
{
  Name = PTC_MATERIAL_TYPE
  Type = Integer
  Default = 9
  Access = Locked
},
{
  Name = PTC_FAILURE_CRITERION_TYPE
  Type = String
  Default = 'NONE'
  Access = Locked
},
{
  Name = PTC_FATIGUE_TYPE
  Type = String
  Default = 'NONE'
  Access = Locked
},
{
  Name = PTC_MATERIAL_SUB_TYPE
  Type = String
  Default = 'LINEAR'
  Access = Locked
},
{
  Name = PTC_YOUNG_MODULUS
  Type = Real
  Default = 2.100000e+02 GPa
  Access = Full
},
{
  Name = PTC_POISSON_RATIO
  Type = Real
  Default = 3.000000e-01
  Access = Full
},
{
  Name = PTC_MASS_DENSITY
  Type = Real
  Default = 7.850000e+00 g/cm^3
  Access = Full
},
{
  Name = PTC_THERMAL_EXPANSION_COEF
  Type = Real
  Default = 1.060000e-05 /C
  Access = Full
},
{
  Name = PTC_THERMAL_CONDUCTIVITY
  Type = Real
  Default = 5.000000e+07 mm g / (sec^3 C)
  Access = Full
},
{
  Name = PTC_SPECIFIC_HEAT
  Type = Real
  Default = 3.000000e-01 mm^2/(sec^2 C)
  Access = Full
},
{
  Name = PTC_CONDITION
  Type = String
  Default = 'Cr12MoV'
  Access = Full
},
{
  Name = PTC_XHATCH_FILE
  Type = String
  Default = 'CR12MOV'
  Access = Full
}

}
