ND_RelParSet_K01 = {

Name = 35CRMO

PARAMETERS =
{
  Name = cmaterial 
  Type = String
  Default = '35CrMo'
  Access = Full
},
{
  Name = PTC_MATERIAL_DESCRIPTION
  Type = String
  Default = '用于制造承受冲击、弯扭、高载荷的各种机器中的重要零件，如轧钢机人字齿轮、曲轴、锤杆、连杆、紧固件，汽轮发动机主轴、车轴，发动机传动零件，大型电动机轴，石油机械中的穿孔器，工作温度低于400摄氏度的锅炉用螺栓，低于510摄氏度的螺母，化工机械中高压无缝厚壁的导管（温度450~500摄氏度，无腐蚀性介质）等；还可代替40CrNi用于制造高载荷传动轴、汽轮发动机转子、大截面齿轮、支承轴（直径小于500MM）等；工艺上的设备材料、管材、焊材等等。'
  Access = Full
},
{
  Name = TEMPERATURE
  Type = Real
  Default = 0.000000e+00 C
  Access = Full
},
{
  Name = PTC_INITIAL_BEND_Y_FACTOR
  Type = Real
  Default = 5.000000e-01
  Access = Full
},
{
  Name = PTC_BEND_TABLE
  Type = String
  Default = ''
  Access = Full
},
{
  Name = PTC_MATERIAL_TYPE
  Type = Integer
  Default = 9
  Access = Locked
},
{
  Name = PTC_FAILURE_CRITERION_TYPE
  Type = String
  Default = 'NONE'
  Access = Locked
},
{
  Name = PTC_FATIGUE_TYPE
  Type = String
  Default = 'NONE'
  Access = Locked
},
{
  Name = PTC_MATERIAL_SUB_TYPE
  Type = String
  Default = 'LINEAR'
  Access = Locked
},
{
  Name = PTC_YOUNG_MODULUS
  Type = Real
  Default = 2.100000e+08 kPa
  Access = Full
},
{
  Name = PTC_POISSON_RATIO
  Type = Real
  Default = 3.000000e-01
  Access = Full
},
{
  Name = SHEAR_MODULUS
  Type = Real
  Default = 7.940000e+07 kPa
  Access = Full
},
{
  Name = PTC_MASS_DENSITY
  Type = Real
  Default = 7.850000e-06 kg/mm^3
  Access = Full
},
{
  Name = PTC_THERMAL_EXPANSION_COEF
  Type = Real
  Default = 1.060000e-05 /C
  Access = Full
},
{
  Name = THERM_EXPANSION_REF_TEMPERATURE
  Type = Real
  Default = 2.000000e+01
  Access = Full
},
{
  Name = STRUCTURAL_DAMPING_COEFFICIENT
  Type = Real
  Default = 1.000000e+01
  Access = Full
},
{
  Name = STRESS_LIMIT_FOR_TENSION
  Type = Real
  Default = 6.850000e+11 kPa
  Access = Full
},
{
  Name = STRESS_LIMIT_FOR_COMPRESSION
  Type = Real
  Default = -6.850000e+11 kPa
  Access = Full
},
{
  Name = STRESS_LIMIT_FOR_SHEAR
  Type = Real
  Default = 3.250000e+11 kPa
  Access = Full
},
{
  Name = PTC_THERMAL_CONDUCTIVITY
  Type = Real
  Default = 5.000000e+04 mm kg /(sec^3 C)
  Access = Full
},
{
  Name = EMISSIVITY
  Type = Real
  Default = 7.000000e-01
  Access = Full
},
{
  Name = PTC_SPECIFIC_HEAT
  Type = Real
  Default = 3.000000e-01 mm^2/(sec^2 C)
  Access = Full
},
{
  Name = PTC_CONDITION
  Type = String
  Default = '调质'
  Access = Full
},
{
  Name = PRO_UNIT_SYS
  Type = String
  Default = 'BOSUN'
  Access = Full
},
{
  Name = PTC_HARDNESS
  Type = Real
  Default = 2.400000e+02
  Access = Full
},
{
  Name = PTC_HARDNESS_TYPE
  Type = String
  Default = 'HB'
  Access = Full
},
{
  Name = PTC_TENSILE_YIELD_STRESS
  Type = Real
  Default = 4.500000e+02 MPa
  Access = Full
},
{
  Name = PTC_TENSILE_ULTIMATE_STRESS
  Type = Real
  Default = 6.500000e+02 MPa
  Access = Full
}

}
