ND_RelParSet_K01 = {

Name = 40CR

PARAMETERS =
{
  Name = cmaterial 
  Type = String
  Default = '40Cr'
  Access = Full
},
{
  Name = PTC_MATERIAL_DESCRIPTION
  Type = String
  Default = '这种钢经调质后用于制造承受中等负荷及中等速度工作的机械零件，如汽车的转向节、后半轴以及机床上的齿轮、轴、蜗杆、花键轴、顶尖套等；经淬火及中温回火后用于制造承受高负荷、冲击及中等速度工作的零件，如齿轮、主轴、油泵转子、滑块、套环等；经淬火及低温回火后用于制造承受重负荷、低冲击及具有耐磨性、截面上实体厚度在25mm以下的零件，如蜗杆、主轴、轴、套环等；经调质并高频表面淬火后用于制造具有高的表面硬度及耐磨性而无很大冲击的零件，如齿轮、套筒、轴、主轴、曲轴、心轴、销子、连杆、 螺钉、螺帽、进气阀等。此外，这种钢又适于制造进行碳氮共渗处理的各种传动零件，如直径较大和低温韧性好的齿轮和轴。'
  Access = Full
},
{
  Name = TEMPERATURE
  Type = Real
  Default = 0.000000e+00 C
  Access = Full
},
{
  Name = PTC_INITIAL_BEND_Y_FACTOR
  Type = Real
  Default = 5.000000e-01
  Access = Full
},
{
  Name = PTC_BEND_TABLE
  Type = String
  Default = ''
  Access = Full
},
{
  Name = PTC_MATERIAL_TYPE
  Type = Integer
  Default = 9
  Access = Locked
},
{
  Name = PTC_FAILURE_CRITERION_TYPE
  Type = String
  Default = 'NONE'
  Access = Locked
},
{
  Name = PTC_FATIGUE_TYPE
  Type = String
  Default = 'NONE'
  Access = Locked
},
{
  Name = PTC_MATERIAL_SUB_TYPE
  Type = String
  Default = 'LINEAR'
  Access = Locked
},
{
  Name = PTC_YOUNG_MODULUS
  Type = Real
  Default = 2.100000e+08 kPa
  Access = Full
},
{
  Name = PTC_POISSON_RATIO
  Type = Real
  Default = 3.000000e-01
  Access = Full
},
{
  Name = SHEAR_MODULUS
  Type = Real
  Default = 7.940000e+07 kPa
  Access = Full
},
{
  Name = PTC_MASS_DENSITY
  Type = Real
  Default = 7.850000e-06 kg/mm^3
  Access = Full
},
{
  Name = PTC_THERMAL_EXPANSION_COEF
  Type = Real
  Default = 1.060000e-05 /C
  Access = Full
},
{
  Name = THERM_EXPANSION_REF_TEMPERATURE
  Type = Real
  Default = 2.000000e+01
  Access = Full
},
{
  Name = STRUCTURAL_DAMPING_COEFFICIENT
  Type = Real
  Default = 1.000000e+01
  Access = Full
},
{
  Name = STRESS_LIMIT_FOR_TENSION
  Type = Real
  Default = 6.850000e+11 kPa
  Access = Full
},
{
  Name = STRESS_LIMIT_FOR_COMPRESSION
  Type = Real
  Default = -6.850000e+11 kPa
  Access = Full
},
{
  Name = STRESS_LIMIT_FOR_SHEAR
  Type = Real
  Default = 3.250000e+11 kPa
  Access = Full
},
{
  Name = PTC_THERMAL_CONDUCTIVITY
  Type = Real
  Default = 5.000000e+04 mm kg /(sec^3 C)
  Access = Full
},
{
  Name = EMISSIVITY
  Type = Real
  Default = 7.000000e-01
  Access = Full
},
{
  Name = PTC_SPECIFIC_HEAT
  Type = Real
  Default = 3.000000e-01 mm^2/(sec^2 C)
  Access = Full
},
{
  Name = PTC_CONDITION
  Type = String
  Default = '调质'
  Access = Full
},
{
  Name = PRO_UNIT_SYS
  Type = String
  Default = 'BOSUN'
  Access = Full
},
{
  Name = PTC_HARDNESS
  Type = Real
  Default = 2.500000e+02
  Access = Full
},
{
  Name = PTC_HARDNESS_TYPE
  Type = String
  Default = 'HB'
  Access = Full
},
{
  Name = PTC_TENSILE_YIELD_STRESS
  Type = Real
  Default = 7.850000e+02 MPa
  Access = Full
},
{
  Name = PTC_TENSILE_ULTIMATE_STRESS
  Type = Real
  Default = 9.800000e+02 MPa
  Access = Full
}

}
