!# Pro/TABLE
!# Pro/TABLE  TM  Version E-03-03  (c) 1988-93 by Parametric Technology Corporation  All Rights Reserved.
! [] S 92;
! [] W 10;
! [A] W 11;
! [B] W  7;
"! Any cell preceeded by ! will be ignored" 
"! Any cell preceeded by # will be treated as a comment" 
"! All comments must be at the beginning of the file before table header" 

"ISO Tolerance table" 

"Table_Type" "Holes" 
"Table_Name" "CD" 
"Table_Unit" "micrometer" 
"Range_Unit" "millimeter" 

"Basic Size" 6 7 8 9 10 

"- -  3" "\"40/34" "\"44/34" "\"48/34" "\"59/34" "\"74/34" 
"3 -  6" "\"54/46" "\"58/46" "\"64/46" "\"76/46" "\"94/46" 
"6 - 10" "\"65/56" "\"71/56" "\"78/56" "\"92/56" "\"114/56" 
