!# Pro/TABLE
!# Pro/TABLE  TM  Version E-03-08  (c) 1988-93 by Parametric Technology Corporation  All Rights Reserved.
! [] S 92;
! [] W 10;
! [A] W 11;
! [G] W 11;
"! Any cell preceeded by ! will be ignored" 
"! Any cell preceeded by # will be treated as a comment" 
"! All comments must be at the beginning of the file before table header" 

"ISO Tolerance table" 

"Table_Type" "General_Dims" 
"Table_Name" "Defaults" 
"Table_Unit" "millimeter" 
"Range_Unit" "millimeter" 					

"Description" "\"0.5 - 3.0" "\"3 - 6" "\"6 - 30" "\"30 - 120" "\"120 - 400" "\"400 - 1000" "\"1000 - 2000" "\"2000 - 4000" 

"Fine" 0.05 0.05 0.1 0.15 0.2 0.3 0.5 "\"-" 
"Medium" 0.1 0.1 0.2 0.3 0.5 0.8 1.2 2 
"Coarse" 0.2 0.3 0.5 0.8 1.2 2 3 4 
"Very Coarse" "\"-" 0.5 1 1.5 2.5 4 6 8 
