!# Pro/TABLE
!# Pro/TABLE  TM  Version E-01-41  (c) 1988-93 by Parametric Technology Corporation  All Rights Reserved.
! [] S 92;
! [] W 10;
! [A] W 11;
"! Any cell preceeded by ! will be ignored" 
"! Any cell preceeded by # will be treated as a comment" 
"! All comments must be at the beginning of the file before table header" 

"ISO Tolerance table" 

"Table_Type" "Broken_Edges" 
"Table_Name" "Defaults" 
"Table_Unit" "millimeter" 
"Range_Unit" "millimeter" 		

"Description" "\"0.5 - 3.0" "\"3 - 6" "\"6 - 4000" 

"Fine" 0.2 0.5 1 
"Medium" 0.2 0.5 1 
"Coarse" 0.4 1 2 
"Very Coarse" 0.4 1 2 
